**LDA ONE Menu Structure**

Firmware v02.00.01.00

# PA OPERATOR

## VOLUME

### Master

#### In1

#### In2

#### In3

#### In 4 mix

## MATRIX

### Select Zone

#### Zone #

##### In 1 (Yes/No)

##### In 2 (Yes/No)

##### BGM (In4-Mix, In 3, None)

## MONITOR

### Zones

#### Select Zone

##### Zone #

###### Source

###### Vumeter

###### Lab (Label)

### Inputs

#### Select Input

##### In 1 (Vumeter/Label)

##### In 2 (Vumeter/Label)

##### In 3 (Vumeter/Label)

##### In 4 Mix (Vumeter)

# VA OPERATOR

## Insert Login L2 (Password 0002)

### Launch EVAC

#### ALL ZONES

#### SINGLE ZONE

##### Zone # (Press Ok)

### Launch ALERT

#### All Zones

#### Single Zone

##### Zone # (Press OK)

### Enter EMG

* + - 1. Press Ok

### Silence Zones

#### All Zones (Press Ok)

#### Single Zone

##### Zone # (Press Ok)

### Reset Zones

#### All Zones (Press Ok)

#### Single Zone

##### Zone # (Press Ok)

### Reset Sys EMG (Press Ok)

### VA Monitor

#### Z#: PA-Idle (or current state)

# SYS MONITOR

## VA Monitor

### Zone #/#

## EMG Log

## FLT Log

## SYS Log

## Logs Config

### See Solved FLT

### View Interval

### Export Logs

### Erase Logs

## Sys Info

### Device

#### Device Addr.

#### Firmware Ver.

#### Bootloader Ver.

#### Serial Number

#### Location

### System

#### System UID

#### Zones Count

#### Devices Count

#### Device Monitor

##### Dev #

###### Dev # Link

###### Dev # Zones

###### Dev # First Z

###### Identify (#)

### Date/Time

## Test

# CONFIGURATION

## AUDIO INPUTS

### Input 1

#### Vumeter

#### PA Volume

#### VA Volume

#### Mute

#### Eq Enable (On/Off)

#### Eq Settings

##### Select Band

###### Freq

###### Gain

###### Width

#### Compressor (On/Off)

#### Override 24 V

#### Trigger Mode

##### Always On

##### TTL Contact Enabled

##### Vox Enable (Noise Gate)

##### Vox Threshold

#### Input 1 Label

### Input 2

#### Vu Meter

#### PA Volume

#### VA Volume

#### Mute

#### Eq Enable (On/Off)

#### Eq Settings

##### Select Band

###### Freq

###### Gain

###### Width

#### Compressor (On/Off)

#### Override 24 V

#### Trigger Mode

##### Always On

##### TTL Contact Enabled

##### Vox Enable (Noise Gate)

##### Vox Threshold

#### Input 2 Label

### Input 3

#### Vu Meter

#### PA Volume

#### VA Volume

#### Mute

#### Eq Enable (On/Off)

#### Eq Settings

##### Select Band

###### Freq

###### Gain

###### Width

#### Compressor (On/Off)

#### Override 24 V

#### Input 3 Label

### Input 4 (mix)

#### Vu Meter

#### PA Volume

#### VA Volume

#### Mute

#### Override 24 V

#### Inputs Select

##### Input 1 (Enabled/Disabled)

##### Input 2 (Enabled/Disabled)

##### Input 3 (Enabled/Disabled)

#### Inputs Volume

##### Input 1

##### Input 2

##### Input 3

#### Mix Fade (dB)

#### Input 4 Label

## AUDIO OUTPUTS

### Amplifier

#### Master PA Vol

#### Master VA Vol

#### Mute (On/Off)

#### Eq Enable

#### Eq Settings

#### Loudness

#### Advanced

##### Amplifier 1

###### Superv: On

###### Gain

###### Temp

##### Amplifier 2

###### Superv: On

###### Gain

###### Temp

##### Common Config

###### Min Temp

###### Max Temp

###### Gain Lower Tol

###### Gain Upper Tol

###### Err. Detect (s)

###### Mode 70 Volts

### Pre-Outputs

#### Select Pre-Out #

##### PA Volume

##### VA Volume

##### Mute

##### Link to Zone

##### Label

### VA Rec-Out

## SPEAKER LINES

### Sel. Spk. Line

#### Line #

##### Line Superv. (On/Off)

##### Line Status

##### Last Measure Z

##### Nominal Z

##### Nominal Z Mute

##### Calibrate

###### Press Ok

##### Lower Tol

##### Upper Tol

##### Owner Zone

##### Owner Z Label

## DEVICE ZONES

### Zones Config

#### Select Zone #

##### Zone # Mute

##### Zone # Label

#### A/B Mode (Off/On)

#### Zones Number

## MESSAGES

### Storage

#### View Playlist

##### Evac

##### Alert

#### Import MSG

##### Select Slot (DATA01, DATA02..)

#### Backup MSG

##### Select Slot (DATA01, DATA02..)

#### Erase MSG (Press Ok)

#### Disk Usage

##### EVAC Playlist

##### Alert Playlist

##### Disk Free Size

##### Disk Full Size

### Player Slot 1

#### Vu Meter

#### VA Volume

#### Eq Enable

#### Eq Settings

### Player Slot 2

#### Vu MEter

#### VA Volume

#### Eq Enable

#### Eq Settings

## ACSI DEVICES

### Monitor

#### ACSI Addr #

##### Disc (Discovered)

##### Inst (Installed)

##### Stat

### Install

#### Addr #: (Vap, MPS8Z, none)

### Input Config

#### Vu Meter

#### Eq Enable

#### Eq Settings

#### Compressor

### MICs Config

#### Select ACSI

##### Vu Meter

##### Volume

##### Override 24V

##### ACSI # Label

## CIE

### Input Status

#### RST: (OpenC/ClosedC)

#### EMG:

#### Z#

### Inputs Config

#### Sel. CIE Input

##### RST

###### Enabled/Disabled

##### EMG

###### EMG Mode (Evac ALL / Alert ALL / Set Sys EMG / Disabled)

##### Z#

###### Enable

###### Superv.

###### N/C Mode

###### Alert Mode

###### Zone Id

### CIE Auto Alert

### CIE Auto Reset

### CIE Local Mode

### Status Out N/C

### RS485 Conf

#### Baud Rate

#### Parity (Even/Odd)

#### Stop Bits

## BATTERY

### Monitor

#### Chg. Status

#### Batt Z (mOhms)

#### Batt Voltage

#### Chg. Curr (mA)

#### Temperature

### Charger Enable

### Supervision

### Temp. Sensor

### Fault Levels

#### Min Voltage

#### Max Imp. mOhms

## LOAD/SAVE

### Import Dev CFG

#### Select Slot

### Export Dev CFG

#### Select Slot

## DEVICE

### Run Autosetup (Press Ok)

#### Import messages? (Yes/No)

##### Erase messages? (Yes/No)

##### Select Slot (DATA #)

##### MSG IMPORT

##### Press OK to view Report

#### Advanced Mode? (Yes/No)

##### Use A/B Lines? (Yes/No)

#### RUNNING AUTOSET.

#### Press OK to view Report

### Restart Device

### Factory Reset

### Fw Update

### Location

#### Location

#### Show On Home

## SYSTEM

### Run Discover (only allowed if LDAONELOOP is installed)

### System Info

#### Device Addr

#### Sys Zone Count

#### Sys Dev Count

#### System UID

### Device Monitor

#### Select Device – Device #

##### Dev # Link

##### Dev # Zones

##### Dev # First Z

##### Identify (#)

### Local Config

#### Bus Baudrate

#### Loopback FLT (Enabled/Disabled)

#### Slave Beep On (Disabled/Enabled)

#### Unlink

### Date/Time

# LOGIN

## INSERT LOGIN

## ACCESS CONFIG

### Pass PA Enable

### Set PA Pass

### Pass L2 Enable

### Set L2 Pass

### Pass L3 Enable

### Set L3 Pass